**A highly effective powerful detergent with built in corrosion inhibitors for hot or cold pressure spray or soak tank cleaning of both ferrous and non ferrous components. The low foam action makes it ideal for spray parts washers.**

* DIRECTIONS FOR USE:

**For general purpose cleaning of transmission parts etc use at a concentration of 0.2% to 0.6% (10-30 grams per 4.5LT).**

**For heavy deposits this can be increased to 1% (45gms /4.5LT)**

Designed for us in spray parts washer machinery and soak tanks.

In all cases wipe dry with a clean cloth or thoroughly rinse clean with water.

* BIODEGRADABLE:

The surfactants in this product are biodegradable according to internationally accepted criteria.

* PRESENTATION:

TURBOWASH Parts Washer Powder is available in:

* 20kg plastic buckets,
* MPI Approved:

MPI C32 APPROVED

* HAZARDS:

**Considered a Hazardous Substance according to the criteria of the New Zealand Hazardous Substances New Organisms legislation.**

**Classified as Dangerous Goods for transport purposes.**

* Harmful if swallowed
* Causes mild skin irritation
* Causes serious eye damage

Wear protective gloves/protective clothing/eye protection/face protection.

* FIRST AID:

**IF IN EYES:**

Rinse cautiously with water for several minutes. Remove contact lenses, if present and easy to do. Continue rinsing.

Immediately call a POISON CENTER/doctor/physician/first aider

**IF SKIN IRRITATION OCCURS:**

Get medical advice/attention.

**IF SWALLOWED:**

Call a POISON CENTER/doctor/physician/first aider/if you feel unwell.

NZ Poisons Centre 0800 POISON (0800 764 766) | NZ Emergency Services: 111

**A Safety Data Sheet is available for this**

**product on request.**.